
Integrated Baseboard Management Controller (iBMC) Firmware Update  README File 


1.0  Installing and Setup Instructions for Web GUI
______________________________________

   1. Copy the this folder to your destination working folder

   2. Log into Web GUI via Web Browser.

   3. Select "Firmware Update" menu of the view.

   4. Select the firmaware image which you need update( "xxxxx.ima") ,then Click "Start firmware update" button for BMC FW update 
   
   5. If you need Preserve Configuration Click "Edit Preserve Configuration" for BMC FW current configuration preserve.

   6. Click "Proceed to Flash" button to start upload.

   7. For a successful upload, the current firmware version and the version of the new
      file will be displayed, as well as the Preserve Configuration show.

   8. Next, click the "Flash selected sections" button and then choose "Full Flash" to begin the firmware update process and view the
      update status. When the update is completed, the embedded software will reboot
      automatically. 
     

2.0  Installing and Setup Instructions for local linux OS with socflash utility
______________________________________

   1. Copy the this folder to your local linux OS
   
   2. Enter into this folder path
   
   3. Run this cmd " ./socflash_x64 -s xxxxx.ima "
   
   4. Then Press 'y' to continue 

